ห้างหุ้นส่วนจำกัด เอส.พี.ซี.ลวดเชื่อมและอุปกรณ์
1684 ชั้น 2 ถนนพหลโยธิน แขวงจันทรเกษม เขตจตุจักร กรุงเทพฯ 10900
โทร. 0-2939-6327	แฟกซ์. 0-2930-3318
http://www.spc-weldingandequipment.com
[bookmark: _GoBack]
[image: Indalco-4043-spec]
image1.jpeg
=z ALLOY 4043 | AlSi5

HEMICAL COMPOSITION

Key FearuRes HEMICAL COMPOSITION _
Designed for welding heat retable base alys —is
and including 6XXX series alloys. AHIMINDIASSOCANON

+ Lower meting point and more ity than 5K | AWS/ASTM AS.10
;:« filler alloys /AS.10M: 2012

iy okl sk it OOy
e 150 18273:2004 Numeral  IEILITE]

= Gotlaposs e oy ovw o the et e
‘widely used welding and brazing alloys LOlE2200e 0

+ Excoluntwhen sespetics e o impariance | ENS73:3

© Noxecorondod o a0 5 anodzod

CHEMICAL
ADVANTAGES CCOMPOSITION (%)

‘Albpostion aluminum MIG wire.
+ Superior vire surface fnishforthe best BT Ferainder
foadabsity and rc porformanco
+ Coimipamisniimgmocsstoprecsay | NECH 4540 50
e O R
+ Statoo theart testing equipment toensur
troubl-foe performance of the wold e B <0 003
+ Manufactured under a quaity system cetfiad to
150 9001 stondord T oo <0001
T oo <002
TYPICAL APPLICATIONS
or wokding 60X aloys, and most cstingoloys | IO - <0001
+ Automotive componants
Cipmipals BT oo 0,005
- 5 -
CCONFORMS TO =2, 0]
+AWS/ASTM AS 10/ 10M2012 e P S
+ ENISO 182732004 Sy
SHIELDING GAS camscica e
+ " 100% Argon
ArgoryHelim Misturss m OGBS o a8 AS 0

« Flow Rate: 30- 50 CFH (14.2-23.6 Unmin) o B e

S
erciam e
M rcooo  ouersoo | scoun) T

) Y I = S

oo 4 S v s 7
L % v et 7
e P A 7 v wwaim s 7
sctza 47 v v warm v v
T R AR A 7z v wmwom v

vsws. v v

See AccuPak Payolf Accessories Pa.25 SN RS




