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YAWATA V-1000 For Severe Earth and Sand Abrasion

E 10UM-G0R

‘Surfncing of cutter knivos, shovol teoth, coal cuttons and parts in petrochomisiey

[Characteristics 1

Heavy-conted rutle type elctrode for highly weas sesistant everlaying an parts subject (0 frictional

abrasion. Not suitable for impact conditions, Cloan and smooth bead appearance with minimal

undercuting, Approximately 160% rocovery. Machinable by geinding ol

Typical Chemical Composition of Deposited Metal (%)

C o
1 »
Typical Hardness of Deposited Metal 1
Vickors (1Y) | Rockwll C GIRO) | Shoro Hont Tooutmont
[ =] 7885 | Aswollel preveat nterpass 350C
[ize & Recommended Current Range (AC or DC +)
DiamotorLangthimm) a0 0 R0
Welding Position Carront 0
23 [ETSI 010 a0

Guideline in Usage

1. Use dry eloetodos oaly. Damp oloetrodos should be ro-drind at 300-350°C for 60 minutos befors

Prchoating at mors than 800TC and posthoating ut 600C e roquired.
8 Chenuered or ribrun eeinforcemont suefacing should bo applid.

B TAMATA sy i o, AYATA s igh g el it .




